1 ./robot\_arm is the start command

2 automatically, output the trajectory of the hand as a output.txt file.

3 I used C++11

4 when I solve the problem, I had some questions, so I wrote those on the EN\_Test ~ .docx

5 the result will change, by how the first joint angles are set.